        AN-SOF ANTENNA SIMULATOR
-------------------------------------------------

Parabolic Cylinder Reflector with a Back-Firing Primary Radiator

Explore the design of a self-resonant parabolic cylinder reflector antenna operating at 890-965 MHz. This study analyzes a back-firing dipole-reflector feed system modeled in AN-SOF, demonstrating how to achieve a stable 50-Ohm match and an asymmetric fan-beam pattern (55° Horizontal, 25° Vertical) without complex matching networks. 